v1
TYPE=0
// code,text,key,diameter,external height,internal height,use the XML position,type (0=neutral / 1=internal / 2=external)

999,"------------------------------"
001,"Vortex 0.4 mm","retypeusc",4.8,0,4.2,no,2
002,"Vortex 0.8 mm","retypeusc",4.8,0,4.3,no,2
003,"Vortex 1.0 mm","retypeusc",4.8,0,4.5,no,2
004,"Vortex 1.2 mm","retypeusc",4.8,0,4.7,no,2
005,"Vortex 1.4 mm","retypeusc",4.8,0,4.9,no,2
999,"------------------------------"
006,"Min Screw Direct MUA","retypeusc",0,0,0,no,2
999,"------------------------------"
018,"PowerBall MUA 2.0 Straight","retypeuzc",0,0,0,no,2
009,"PowerBall SRA 1.0","retypeuzc",0,0,0,no,2
008,"PowerBall MUA 2.0","retypeuzc",0,0,0,no,2
007,"PowerBall MB 2.0","retypeuzc",0,0,0,no,2
999,"------------------------------"
012,"RosenScrew 1.4","ec",0,0,0,no,2
011,"RosenScrew 1.6","ec",0,0,0,no,2
010,"RosenScrew 1.7","ec",0,0,0,no,2
999,"------------------------------"
025,"SegScrew MUA V1.1.3 100um","ec",4.9,4,4,no,2
024,"SegScrew MUA V1.1.3 80um","ec",4.9,4,4,no,2
023,"SegScrew MUA V1.1.3 60um","ec",4.9,4,4,no,2
022,"SegScrew MUA V1.1.3 50um","ec",4.9,4,4,no,2
021,"SegScrew MUA V1.1.3 40um","ec",4.9,4,4,no,2
020,"SegScrew MUA V1.1.3 30um","ec",4.9,4,4,no,2
019,"SegScrew MUA V1.1.3 20um","ec",4.9,4,4,no,2
999,"------------------------------"
026,"Mini Pilar 3D","retypeusc",0,0,0,no,2
999,"-- Badger Screw MU RP --"
013,"Badger Screw MU RP","retypeusc",4.8,0,4.8,no,2


// INSTRUCTIONS FOR SETUP:
// Curve Name Requirements: Always starts with "r" (replace) and ends with "c" (looks for this letter in the ending. Also cannot end the name of a curve with "cc")
// 2nd Letter is "i" for Internal Interface or "e" for External Interface
// 3-6 Letters is used for a short abbreviation of the Implant System (IE: 3i - "trei" Italiano, Ankylos Anti-Rotative - "anka", Ankylos Rotative - "ankr" 
// 7th Letter is used for Implant Sizes (IE: 3.0 = "a", 3.5mm = "b", 4.0 = "d", 6.0 = "e". NOTE: "c" is skipped because we have to end the curve name with a single "c" as stated above.
// 8th Letter always ends with "c"
// Make sure to place the Surfaces and any curves into the -DM-W- Layer within Rhino / SUM3D - Remove any unused layers
// When Importing Geometry into SUM3D, use Alt+Enter+909
// Tutti i ROT alla fine mettere 2, cosi SUM si comporta come se fossi una interfaccia External
